|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  |  | |
|  | REPAIR UPDATES – 7/11/24 | | |  | |  |
| Address | Description and diagnosis | | | Status | | Repair Date |
| 389 E. Palm Lane | 1. Resealed stand box location at S/E corner of the lot in alley. 2. Demo & remove stand box, saw cut and remove 10x23 concrete pipe. Install 12-15'x12" 80#PIP using proper adaptations and bonding material. | | | Repaired | | 1/23/2024 & 2/19/24 |
| 357 E. Monte Vista | Repair broken joint/ring crack. Reset pipe and backfill. | | | Repaired | | 1/23/2024 |
| 360 E. Monte Vista | Replaced old toggle gates with new gates and 3’ handle extensions. | | | Repaired | | 1/24/2024 |
| 124 E. Palm Lane | Replaced deficient gate from stand box and installed new gate with handle extension | | | Repaired | | 1/24/2024 |
| 371 E. Monte Vista | Replaced valve stem. | | | Repaired | | 2/1/2024 |
| 2024 N 7th St. | Remove 2x pipe gates from standbox. Install 2x new 10"x5' HDPD using concrete anchors and hydraulic rapid set. | | | Repaired | | 2/19/2024 |
| 2034 N. 3rd St. | Repair broken joint/ring crack. Reset pipe and backfill. | | | Repaired | | 4/12/2024 |
| 2016 N. Alvarado | Repair broken joint/ring crack. Reset pipe and backfill. | | | Repaired | | 4/22/2024 |